{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":147,"n_cols":15,"rows_kept":147,"merged":[[0,0,0,14],[83,0,83,14]]}
["XLY6ULL-CORE V1.0引脚分配表J1"]
["引脚号","CPU管脚","网络标号","默认功能描述","CPU管脚名称","功能零","功能一","功能二","功能三","功能四","功能五","功能六","功能七","功能八","功能九"]
[1,"K17","ENET_MDIO","RMII1 MDIO数据","GPIO1_IO06","ENET1_MDIO","ENET2_MDIO","USB_OTG_PWR_WAKE","CSI_MCLK","USDHC2_WP","GPIO1_IO06","CCM_WAIT","CCM_REF_EN_B","UART1_CTS_B"]
[2,"L16","ENET_MDC","RMII1 MDIO时钟","GPIO1_IO07","ENET1_MDC","ENET2_MDC","USB_OTG_HOST_MODE","CSI_PIXCLK","USDHC2_CD_B","GPIO1_IO07","CCM_STOP",null,"UART1_RTS_B"]
[3,"E17","ENET1_RXD1","RMII1接收数据1","ENET1_RX_DATA1","ENET1_RDATA01","UART4_CTS_B","PWM2_OUT","CSI_DATA17","FLEXCAN1_RX","GPIO2_IO01","KPP_COL00",null,"USDHC2_LCTL","EPDC_SDCE05(ULL)"]
[4,"C16","ENET2_RXD1","RMII2 接收数据1","ENET2_RX_DATA1","ENET2_RDATA01","UART6_RX","SIM1_PORT0_CLK(UL)","I2C3_SDA","ENET1_MDC","GPIO2_IO09","KPP_COL04",null,"USB_OTG1_OC","EPDC_SDDO09(ULL)"]
[5,"F16","ENET1_RXD0","RMII1接收数据0","ENET1_RX_DATA0","ENET1_RDATA00","UART4_RTS_B","PWM1_OUT","CSI_DATA16","FLEXCAN1_TX","GPIO2_IO00","KPP_ROW00",null,"USDHC1_LCTL","EPDC_SDCE04(ULL)"]
[6,"C17","ENET2_RXD0","RMII2 接收数据0","ENET2_RX_DATA0","ENET2_RDATA00","UART6_TX","SIM1_PORT0_TRXD(UL)","I2C3_SCL","ENET1_MDIO","GPIO2_IO08","KPP_ROW04",null,"USB_OTG1_PWR","EPDC_SDDO08(ULL)"]
[7,"E16","ENET1_CRS_DV","RMII1 CRSDV","ENET1_RX_EN","ENET1_RX_EN","UART5_RTS_B","OSC32K_32K_OUT(UL)","CSI_DATA18","FLEXCAN2_TX","GPIO2_IO02","KPP_ROW01",null,"USDHC1_VSELECT","EPDC_SDCE06(ULL)"]
[8,"B17","ENET2_CRS_DV","RMII2 CRSDV","ENET2_RX_EN","ENET2_RX_EN","UART7_TX","SIM1_PORT0_RST_B(UL)","I2C4_SCL","EIM_ADDR26","GPIO2_IO10","KPP_ROW05",null,"ENET1_REF_CLK_25M","EPDC_SDDO10(ULL)"]
[9,"D15","ENET1_RXER","RMII1 RXER","ENET1_RX_ER","ENET1_RX_ER","UART7_RTS_B","PWM8_OUT","CSI_DATA23","EIM_CRE","GPIO2_IO07","KPP_COL03",null,"GPT1_CAPTURE2","EPDC_SDOEZ(ULL)"]
[10,"D16","ENET2_RXER","RMII2 RXER","ENET2_RX_ER","ENET2_RX_ER","UART8_RTS_B","SIM2_PORT0_SVEN(UL)","ECSPI4_SS0","EIM_ADDR25","GPIO2_IO15","KPP_COL07",null,"WDOG1_WDOG_ANY","EPDC_SDDO15(ULL)"]
[11,"E14","ENET1_TXD1","RMII1发送数据1","ENET1_TX_DATA1","ENET1_TDATA01","UART6_CTS_B","PWM5_OUT","CSI_DATA20","ENET2_MDIO","GPIO2_IO04","KPP_ROW02",null,"WDOG1_WDOG_RST_B_DEB","EPDC_SDCE08(ULL)"]
[12,"A16","ENET2_TXD1","RMII2 发送数据1","ENET2_TX_DATA1","ENET2_TDATA01","UART8_TX","SIM2_PORT0_TRXD(UL)","ECSPI4_SCLK","EIM_EB_B03","GPIO2_IO12","KPP_ROW06",null,"USB_OTG2_PWR","EPDC_SDDO12(ULL)"]
[13,"E15","ENET1_TXD0","RMII1发送数据0","ENET1_TX_DATA0","ENET1_TDATA00","UART5_CTS_B","ANATOP_24M_OUT(UL)","CSI_DATA19","FLEXCAN2_RX","GPIO2_IO03","KPP_COL01",null,"USDHC2_VSELECT","EPDC_SDCE07(ULL)"]
[14,"A15","ENET2_TXD0","RMII2 发送数据0","ENET2_TX_DATA0","ENET2_TDATA00","UART7_RX","SIM1_PORT0_SVEN(UL)","I2C4_SDA","EIM_EB_B02","GPIO2_IO11","KPP_COL05",null,null,"EPDC_SDDO11(ULL)"]
[15,"F15","ENET1_TXEN","RMII1 TXEN","ENET1_TX_EN","ENET1_TX_EN","UART6_RTS_B","PWM6_OUT","CSI_DATA21","ENET2_MDC","GPIO2_IO05","KPP_COL02",null,"WDOG2_WDOG_RST_B_DEB","EPDC_SDCE09(ULL)"]
[16,"B15","ENET2_TXEN","RMII2 TXEN","ENET2_TX_EN","ENET2_TX_EN","UART8_RX","SIM2_PORT0_CLK(UL)","ECSPI4_MOSI","EIM_ACLK_FREERUN","GPIO2_IO13","KPP_COL06",null,"USB_OTG2_OC","EPDC_SDDO13(ULL)"]
[17,"F14","ENET1_TX_CLK","RMII1时钟","ENET1_TX_CLK","ENET1_TX_CLK","UART7_CTS_B","PWM7_OUT","CSI_DATA22","ENET1_REF_CLK1","GPIO2_IO06","KPP_ROW03",null,"GPT1_CLK","EPDC_SDOED(ULL)"]
[18,"D17","ENET2_TX_CLK","RMII2时钟","ENET2_TX_CLK","ENET2_TX_CLK","UART8_CTS_B","SIM2_PORT0_RST_B(UL)","ECSPI4_MISO","ENET2_REF_CLK2","GPIO2_IO14","KPP_ROW07",null,"ANATOP_OTG2_ID","EPDC_SDDO14(ULL)"]
[19,null,"GND","系统地"]
[20,null,"GND","系统地"]
[21,"B16","LCD_DATA23","LCD数据位23","LCD_DATA23","LCDIF_DATA23","MQS_LEFT","ECSPI1_MISO","CSI_DATA15","EIM_DATA15","GPIO3_IO28","SRC_BT_CFG31",null,"USDHC2_DATA3","EPDC_SDCE03(ULL)"]
[22,"A14","LCD_DATA22","LCD数据位22","LCD_DATA22","LCDIF_DATA22","MQS_RIGHT","ECSPI1_MOSI","CSI_DATA14","EIM_DATA14","GPIO3_IO27","SRC_BT_CFG30",null,"USDHC2_DATA2","EPDC_SDCE02(ULL)"]
[23,"B13","LCD_DATA17","LCD数据位17","LCD_DATA17","LCDIF_DATA17","UART7_RX",null,"CSI_DATA00","EIM_DATA09","GPIO3_IO22","SRC_BT_CFG25",null,"USDHC2_DATA7","EPDC_GDSP(ULL)"]
[24,"C13","LCD_DATA16","LCD数据位16","LCD_DATA16","LCDIF_DATA16","UART7_TX",null,"CSI_DATA01","EIM_DATA08","GPIO3_IO21","SRC_BT_CFG24",null,"USDHC2_DATA6","EPDC_GDOE(ULL)"]
[25,"B14","LCD_DATA21","LCD数据位21","LCD_DATA21","LCDIF_DATA21","UART8_RX","ECSPI1_SS0","CSI_DATA13","EIM_DATA13","GPIO3_IO26","SRC_BT_CFG29",null,"USDHC2_DATA1","EPDC_SDCE01(ULL)"]
[26,"C14","LCD_DATA20","LCD数据位20","LCD_DATA20","LCDIF_DATA20","UART8_TX","ECSPI1_SCLK","CSI_DATA12","EIM_DATA12","GPIO3_IO25","SRC_BT_CFG28",null,"USDHC2_DATA0","EPDC_VCOM01(ULL)"]
[27,"D14","LCD_DATA19","LCD数据位19","LCD_DATA19","LCDIF_DATA19","PWM6_OUT","WDOG1_WDOG_ANY","CSI_DATA11","EIM_DATA11","GPIO3_IO24","SRC_BT_CFG27",null,"USDHC2_CLK","EPDC_VCOM00(ULL)"]
[28,"A13","LCD_DATA18","LCD数据位18","LCD_DATA18","LCDIF_DATA18","PWM5_OUT","CA7_MX6UL_EVENTO","CSI_DATA10","EIM_DATA10","GPIO3_IO23","SRC_BT_CFG26",null,"USDHC2_CMD","EPDC_BDR01(ULL)"]
[29,"D13","LCD_DATA15","LCD数据位15","LCD_DATA15","LCDIF_DATA15","SAI3_TX_DATA",null,"CSI_DATA23","EIM_DATA07","GPIO3_IO20","SRC_BT_CFG15",null,"USDHC2_DATA5","EPDC_GDRL(ULL)"]
[30,"A12","LCD_DATA14","LCD数据位14","LCD_DATA14","LCDIF_DATA14","SAI3_RX_DATA",null,"CSI_DATA22","EIM_DATA06","GPIO3_IO19","SRC_BT_CFG14",null,"USDHC2_DATA4","EPDC_SDSHR(ULL)"]
[31,"B12","LCD_DATA13","LCD数据位13","LCD_DATA13","LCDIF_DATA13","SAI3_TX_BCLK",null,"CSI_DATA21","EIM_DATA05","GPIO3_IO18","SRC_BT_CFG13",null,"USDHC2_RESET_B","EPDC_BDR00(ULL)"]
[32,"C12","LCD_DATA12","LCD数据位12","LCD_DATA12","LCDIF_DATA12","SAI3_TX_SYNC",null,"CSI_DATA20","EIM_DATA04","GPIO3_IO17","SRC_BT_CFG12",null,"ECSPI1_RDY","EPDC_PWRCTRL00(ULL)"]
[33,"D12","LCD_DATA11","LCD数据位11","LCD_DATA11","LCDIF_DATA11","SAI3_RX_BCLK",null,"CSI_DATA19","EIM_DATA03","GPIO3_IO16","SRC_BT_CFG11",null,"FLEXCAN2_RX","EPDC_PWRSTAT(ULL)"]
[34,"E12","LCD_DATA10","LCD数据位10","LCD_DATA10","LCDIF_DATA10","SAI3_RX_SYNC",null,"CSI_DATA18","EIM_DATA02","GPIO3_IO15","SRC_BT_CFG10",null,"FLEXCAN2_TX","EPDC_PWRCOM(ULL)"]
[35,"A11","LCD_DATA9","LCD数据位9","LCD_DATA09","LCDIF_DATA09","SAI3_MCLK",null,"CSI_DATA17","EIM_DATA01","GPIO3_IO14","SRC_BT_CFG09",null,"FLEXCAN1_RX","EPDC_PWRWAKE(ULL)"]
[36,"B11","LCD_DATA8","LCD数据位8","LCD_DATA08","LCDIF_DATA08","SPDIF_IN",null,"CSI_DATA16","EIM_DATA00","GPIO3_IO13","SRC_BT_CFG08",null,"FLEXCAN1_TX","EPDC_PWRIRQ(ULL)"]
[37,"D11","LCD_DATA7","LCD数据位7","LCD_DATA07","LCDIF_DATA07","UART7_RTS_B",null,"ENET2_1588_EVENT3_OUT","SPDIF_EXT_CLK","GPIO3_IO12","SRC_BT_CFG07",null,"ECSPI1_SS3","EPDC_SDDO07(ULL)"]
[38,"A10","LCD_DATA6","LCD数据位6","LCD_DATA06","LCDIF_DATA06","UART7_CTS_B",null,"ENET2_1588_EVENT3_IN","SPDIF_LOCK","GPIO3_IO11","SRC_BT_CFG06",null,"ECSPI1_SS2","EPDC_SDDO06(ULL)"]
[39,"B10","LCD_DATA5","LCD数据位5","LCD_DATA05","LCDIF_DATA05","UART8_RTS_B",null,"ENET2_1588_EVENT2_OUT","SPDIF_OUT","GPIO3_IO10","SRC_BT_CFG05",null,"ECSPI1_SS1","EPDC_SDDO05(ULL)"]
[40,"C10","LCD_DATA4","LCD数据位4","LCD_DATA04","LCDIF_DATA04","UART8_CTS_B",null,"ENET2_1588_EVENT2_IN","SPDIF_SR_CLK","GPIO3_IO09","SRC_BT_CFG04",null,"SAI1_TX_DATA","EPDC_SDDO04(ULL)"]
[41,"D10","LCD_DATA3","LCD数据位3","LCD_DATA03","LCDIF_DATA03","PWM4_OUT",null,"ENET1_1588_EVENT3_OUT","I2C4_SCL","GPIO3_IO08","SRC_BT_CFG03",null,"SAI1_RX_DATA","EPDC_SDDO03(ULL)"]
[42,"E10","LCD_DATA2","LCD数据位2","LCD_DATA02","LCDIF_DATA02","PWM3_OUT",null,"ENET1_1588_EVENT3_IN","I2C4_SDA","GPIO3_IO07","SRC_BT_CFG02",null,"SAI1_TX_BCLK","EPDC_SDDO02(ULL)"]
[43,"A9","LCD_DATA1","LCD数据位1","LCD_DATA01","LCDIF_DATA01","PWM2_OUT",null,"ENET1_1588_EVENT2_OUT","I2C3_SCL","GPIO3_IO06","SRC_BT_CFG01",null,"SAI1_TX_SYNC","EPDC_SDDO01(ULL)"]
[44,"B9","LCD_DATA0","LCD数据位0","LCD_DATA00","LCDIF_DATA00","PWM1_OUT",null,"ENET1_1588_EVENT2_IN","I2C3_SDA","GPIO3_IO05","SRC_BT_CFG00",null,"SAI1_MCLK","EPDC_SDDO00(ULL)"]
[45,null,"GND","系统地"]
[46,null,"GND","系统地"]
[47,"A8","LCD_PCLK","LCD像素时钟","LCD_CLK","LCDIF_CLK","LCDIF_WR_RWN","UART4_TX","SAI3_MCLK","EIM_CS2_B","GPIO3_IO00",null,null,"WDOG1_WDOG_RST_B_DEB","EPDC_SDCLK(ULL)"]
[48,"D9","LCD_HSYNC","LCD水平同步","LCD_HSYNC","LCDIF_HSYNC","LCDIF_RS","UART4_CTS_B","SAI3_TX_BCLK","WDOG3_WDOG_RST_B_DEB","GPIO3_IO02",null,null,"ECSPI2_SS1","EPDC_SDOE(ULL)"]
[49,"B8","LCD_DE","LCD数据使能","LCD_ENABLE","LCDIF_ENABLE","LCDIF_RD_E","UART4_RX","SAI3_TX_SYNC","EIM_CS3_B","GPIO3_IO01",null,null,"ECSPI2_RDY","EPDC_SDLE(ULL)"]
[50,"C9","LCD_VSYNC","LCD垂直同步","LCD_VSYNC","LCDIF_VSYNC","LCDIF_BUSY","UART4_RTS_B","SAI3_RX_DATA","WDOG2_WDOG_B","GPIO3_IO03",null,null,"ECSPI2_SS2","EPDC_SDCE00(ULL)"]
[51,"E9","LCD_PWREN","LCD电源使能","LCD_RESET","LCDIF_RESET","LCDIF_CS","CA7_MX6UL_EVENTI","SAI3_TX_DATA","WDOG1_WDOG_ANY","GPIO3_IO04",null,null,"ECSPI2_SS3","EPDC_GDOE(ULL)"]
[52,null,"GND","系统地"]
[53,null,"NOP"]
[54,null,"NOP"]
[55,"B5","NAND_nCE1","GPIO","NAND_CE1_B","RAWNAND_CE1_B","USDHC1_DATA6","QSPI_A_DATA02","ECSPI3_MOSI","EIM_ADDR18","GPIO4_IO14",null,null,"UART3_CTS_B"]
[56,"E6","RUN_LED","运行指示灯","NAND_DQS","RAWNAND_DQS","CSI_FIELD","QSPI_A_SS0_B","PWM5_OUT","EIM_WAIT","GPIO4_IO16","SDMA_EXT_EVENT01",null,"SPDIF_EXT_CLK"]
[57,"F5","CSI_MCLK","CSI主时钟","CSI_MCLK","CSI_MCLK","USDHC2_CD_B","RAWNAND_CE2_B","I2C1_SDA","EIM_CS0_B","GPIO4_IO17","SNVS_HP_VIO_5_CTL",null,"UART6_TX","ESAI_TX3_RX2(ULL)"]
[58,"J14","SD1_CD","SD1 CD","UART1_RTS_B","UART1_RTS_B","ENET1_TX_ER","USDHC1_CD_B","CSI_DATA05","ENET2_1588_EVENT1_OUT","GPIO1_IO19",null,null,"USDHC2_CD_B","UART5_RTS_B(ULL)"]
[59,"E5","CSI_PIXCLK","CSI像素时钟","CSI_PIXCLK","CSI_PIXCLK","USDHC2_WP","RAWNAND_CE3_B","I2C1_SCL","EIM_OE","GPIO4_IO18","SNVS_HP_VIO_5",null,"UART6_RX","ESAI_TX2_RX3(ULL)"]
[60,"K15","UART1_CTS",null,"UART1_CTS_B","UART1_CTS_B","ENET1_RX_CLK","USDHC1_WP","CSI_DATA04","ENET2_1588_EVENT1_IN","GPIO1_IO18",null,null,"USDHC2_WP","UART5_CTS_B(ULL)"]
[61,"F2","CSI_VSYNC","CSI垂直同步","CSI_VSYNC","CSI_VSYNC","USDHC2_CLK","SIM1_PORT1_CLK(UL)","I2C2_SDA","EIM_RW","GPIO4_IO19","PWM7_OUT",null,"UART6_RTS_B","ESAI_TX4_RX1(ULL)"]
[62,"C1","SD1_CLK","SD1 CLK","SD1_CLK","USDHC1_CLK","GPT2_COMPARE2","SAI2_MCLK","SPDIF_IN","EIM_ADDR20","GPIO2_IO17",null,null,"USB_OTG1_OC"]
[63,"F3","CSI_HSYNC","CSI水平同步","CSI_HSYNC","CSI_HSYNC","USDHC2_CMD","SIM1_PORT1_PD(UL)","I2C2_SCL","EIM_LBA_B","GPIO4_IO20","PWM8_OUT",null,"UART6_CTS_B","ESAI_TX1(ULL)"]
[64,"C2","SD1_CMD","SD1 CMD","SD1_CMD","USDHC1_CMD","GPT2_COMPARE1","SAI2_RX_SYNC","SPDIF_OUT","EIM_ADDR19","GPIO2_IO16","SDMA_EXT_EVENT00",null,"USB_OTG1_PWR"]
[65,"E4","CSI_DATA0","CSI数据0","CSI_DATA00","CSI_DATA02","USDHC2_DATA0","SIM1_PORT1_RST_B(UL)","ECSPI2_SCLK","EIM_AD00","GPIO4_IO21","SRC_INT_BOOT",null,"UART5_TX","ESAI_TX_HF_CLK(ULL)"]
[66,"B3","SD1_DATA0","SD1数据0","SD1_DATA0","USDHC1_DATA0","GPT2_COMPARE3","SAI2_TX_SYNC","FLEXCAN1_TX","EIM_ADDR21","GPIO2_IO18",null,null,"ANATOP_OTG1_ID"]
[67,"E3","CSI_DATA1","CSI数据1","CSI_DATA01","CSI_DATA03","USDHC2_DATA1","SIM1_PORT1_SVEN(UL)","ECSPI2_SS0","EIM_AD01","GPIO4_IO22","SAI1_MCLK",null,"UART5_RX","ESAI_RX_HF_CLK (ULL)"]
[68,"B2","SD1_DATA1","SD1数据1","SD1_DATA1","USDHC1_DATA1","GPT2_CLK","SAI2_TX_BCLK","FLEXCAN1_RX","EIM_ADDR22","GPIO2_IO19",null,null,"USB_OTG2_PWR"]
[69,"E2","CSI_DATA2","CSI数据2","CSI_DATA02","CSI_DATA04","USDHC2_DATA2","SIM1_PORT1_TRXD(UL)","ECSPI2_MOSI","EIM_AD02","GPIO4_IO23","SAI1_RX_SYNC",null,"UART5_RTS_B","ESAI_RX_FS(ULL)"]
[70,"B1","SD1_DATA2","SD1数据2","SD1_DATA2","USDHC1_DATA2","GPT2_CAPTURE1","SAI2_RX_DATA","FLEXCAN2_TX","EIM_ADDR23","GPIO2_IO20","CCM_CLKO1",null,"USB_OTG2_OC"]
[71,"E1","CSI_DATA3","CSI数据3","CSI_DATA03","CSI_DATA05","USDHC2_DATA3","SIM2_PORT1_PD(UL)","ECSPI2_MISO","EIM_AD03","GPIO4_IO24","SAI1_RX_BCLK",null,"UART5_CTS_B","ESAI_RX_CLK(ULL)"]
[72,"A2","SD1_DATA3","SD1数据3","SD1_DATA3","USDHC1_DATA3","GPT2_CAPTURE2","SAI2_TX_DATA","FLEXCAN2_RX","EIM_ADDR24","GPIO2_IO21","CCM_CLKO2",null,"ANATOP_OTG2_ID"]
[73,"D4","CSI_DATA4","CSI数据4","CSI_DATA04","CSI_DATA06","USDHC2_DATA4","SIM2_PORT1_CLK(UL)","ECSPI1_SCLK","EIM_AD04","GPIO4_IO25","SAI1_TX_SYNC",null,"USDHC1_WP","ESAI_TX_FS(ULL)"]
[74,"D3","CSI_DATA5","CSI数据5","CSI_DATA05","CSI_DATA07","USDHC2_DATA5","SIM2_PORT1_RST_B(UL)","ECSPI1_SS0","EIM_AD05","GPIO4_IO26","SAI1_TX_BCLK",null,"USDHC1_CD_B","ESAI_TX_CLK(ULL)"]
[75,"D2","CSI_DATA6","CSI数据6","CSI_DATA06","CSI_DATA08","USDHC2_DATA6","SIM2_PORT1_SVEN(UL)","ECSPI1_MOSI","EIM_AD06","GPIO4_IO27","SAI1_RX_DATA",null,"USDHC1_RESET_B","ESAI_TX5_RX0(ULL)"]
[76,"D1","CSI_DATA7","CSI数据7","CSI_DATA07","CSI_DATA09","USDHC2_DATA7","SIM2_PORT1_TRXD(UL)","ECSPI1_MISO","EIM_AD07","GPIO4_IO28","SAI1_TX_DATA",null,"USDHC1_VSELECT","ESAI_TX0(ULL)"]
[77,null,"GND","系统地"]
[78,null,"VSYS","5V电源输入"]
[79,null,"GND","系统地"]
[80,null,"VSYS","5V电源输入"]
[]
["XLY6ULL-CORE V1.0引脚分配表J2"]
["引脚号","CPU管脚","网络标号","默认功能描述","CPU管脚名称","功能零","功能一","功能二","功能三","功能四","功能五","功能六","功能七","功能八","功能九"]
[1,"T10","BOOT_MODE0","启动模式选择","BOOT_MODE0",{"$nulls":5},"GPIO5_IO10"]
[2,"U10","BOOT_MODE1","启动模式选择","BOOT_MODE1",{"$nulls":5},"GPIO5_IO11"]
[3,null,"nRST_OUT","主板复位输出"]
[4,null,"nRST_IN","外部复位输入"]
[5]
[6,"R8","ONOFF","开关机按钮","ONOFF"]
[7,"H15","CAN1_TX","CAN1发送","UART3_CTS_B","UART3_CTS_B","ENET2_RX_CLK","FLEXCAN1_TX","CSI_DATA10","ENET1_1588_EVENT1_IN","GPIO1_IO26",null,null,"EPIT2_OUT"]
[8,"G14","CAN1_RX","CAN1接收","UART3_RTS_B","UART3_RTS_B","ENET2_TX_ER","FLEXCAN1_RX","CSI_DATA11","ENET1_1588_EVENT1_OUT","GPIO1_IO27",null,null,"WDOG1_WDOG_B"]
[9,"J15","CAN2_TX","CAN2发送","UART2_CTS_B","UART2_CTS_B","ENET1_CRS","FLEXCAN2_TX","CSI_DATA08","GPT1_COMPARE2","GPIO1_IO22",null,"SJC_DE_B","ECSPI3_MOSI"]
[10,"H14","CAN2_RX","CAN2接收","UART2_RTS_B","UART2_RTS_B","ENET1_COL","FLEXCAN2_RX","CSI_DATA09","GPT1_COMPARE3","GPIO1_IO23",null,"SJC_FAIL","ECSPI3_MISO"]
[11,"R6","SNVS_TAMPER9",null,"SNVS_TAMPER9",{"$nulls":5},"GPIO5_IO09"]
[12,"R9","SNVS_TAMPER1",null,"SNVS_TAMPER1",{"$nulls":5},"GPIO5_IO01"]
[13,"N9","SNVS_TAMPER8",null,"SNVS_TAMPER8",{"$nulls":5},"GPIO05_IO08"]
[14,"P11","SNVS_TAMPER2",null,"SNVS_TAMPER2",{"$nulls":5},"GPIO5_IO02"]
[15,"N8","SNVS_TAMPER5",null,"SNVS_TAMPER5",{"$nulls":5},"GPIO5_IO05"]
[16,"P9","SNVS_TAMPER4",null,"SNVS_TAMPER4",{"$nulls":5},"GPIO5_IO04"]
[17,"N10","SNVS_TAMPER7",null,"SNVS_TAMPER7",{"$nulls":5},"GPIO5_IO07"]
[18,"P10","SNVS_TAMPER3",null,"SNVS_TAMPER3",{"$nulls":5},"GPIO5_IO03"]
[19,"N11","SNVS_TAMPER6",null,"SNVS_TAMPER6",{"$nulls":5},"GPIO5_IO06"]
[20,null,"GND","系统地"]
[21,"T12","USB_OTG1_VBUS","USB1VBUS电源","USB_OTG1_VBUS"]
[22,"U12","USB_OTG2_VBUS","USB2VBUS电源","USB_OTG2_VBUS"]
[23,"K13","USB_OTG1_ID","USB1 ID引脚","GPIO1_IO00","I2C2_SCL","GPT1_CAPTURE1","ANATOP_OTG1_ID","ENET1_REF_CLK1","MQS_RIGHT","GPIO1_IO00","ENET1_1588_EVENT0_IN","SRC_SYSTEM_RESET","WDOG3_WDOG_B"]
[24,"M17","USB_OTG2_ID","USB2 ID引脚","GPIO1_IO05","ENET2_REF_CLK2","PWM4_OUT","ANATOP_OTG2_ID","CSI_FIELD","USDHC1_VSELECT","GPIO1_IO05","ENET2_1588_EVENT0_OUT",null,"UART5_RX"]
[25,"T15","USB_OTG1_DN","USB1DN","USB_OTG1_DN"]
[26,"T13","USB_OTG2_DN","USB2DN","USB_OTG2_DN"]
[27,"U15","USB_OTG1_DP","USB1DP","USB_OTG1_DP"]
[28,"U13","USB_OTG2_DP","USB2DP","USB_OTG2_DP"]
[29,"U16","nUSB_OTG_CHD",null,"USB_OTG1_CHD_B"]
[30,null,"GND","系统地"]
[31,null,"GND","系统地"]
[32,"M14","JTAG_TCK","SAI2_RX_DATA","JTAG_TCK","SJC_TCK","GPT2_COMPARE2","SAI2_RX_DATA",null,"PWM7_OUT","GPIO1_IO14","OSC32K_32K_OUT(UL)",null,"SIM2_POWER_FAIL"]
[33,"U9","PMIC_ON_REQ","PMIC_ON_REQ","PMIC_ON_REQ"]
[34,"N14","JTAG_nTRST","SAI2_TX_DATA","JTAG_TRST_B","SJC_TRSTB","GPT2_COMPARE3","SAI2_TX_DATA",null,"PWM8_OUT","GPIO1_IO15","ANATOP_24M_OUT(UL)",null,"CAAM_RNG_OSC_OBS"]
[35,"P16","CLK1_N",null,"CCM_CLK1_N"]
[36,"P14","JTAG_TMS","SAI2_MCLK","JTAG_TMS","SJC_TMS","GPT2_CAPTURE1","SAI2_MCLK","CCM_CLKO1","CCM_WAIT","GPIO1_IO11","SDMA_EXT_EVENT01",null,"EPIT1_OUT"]
[37,"P17","CLK1_P",null,"CCM_CLK1_P"]
[38,"N16","JTAG_TDI","SAI2_TX_BCLK","JTAG_TDI","SJC_TDI","GPT2_COMPARE1","SAI2_TX_BCLK",null,"PWM6_OUT","GPIO1_IO13","MQS_LEFT",null,"SIM1_POWER_FAIL"]
[39,"M15","BEEP","蜂鸣器控制","GPIO1_IO09","PWM2_OUT","WDOG1_WDOG_ANY","SPDIF_IN","CSI_HSYNC","USDHC2_RESET_B","GPIO1_IO09","USDHC1_RESET_B",null,"UART5_CTS_B"]
[40,"N15","JTAG_TDO","SAI2_TX_SYNC","JTAG_TDO","SJC_TDO","GPT2_CAPTURE2","SAI2_TX_SYNC","CCM_CLKO2","CCM_STOP","GPIO1_IO12","MQS_RIGHT",null,"EPIT2_OUT"]
[41,"N17","LCD_BRIGHT","LCD背光亮度PWM","GPIO1_IO08","PWM1_OUT","WDOG1_WDOG_B","SPDIF_OUT","CSI_VSYNC","USDHC2_VSELECT","GPIO1_IO08","CCM_PMIC_RDY",null,"UART5_RTS_B"]
[42,"P15","JTAG_MOD","JTAG MOD","JTAG_MOD","SJC_MOD","GPT2_CLK","SPDIF_OUT","ENET1_REF_CLK_25M","CCM_PMIC_RDY","GPIO1_IO10","SDMA_EXT_EVENT00"]
[43,"L13","VDDA_ADC_3P3","ADC 3.3V参考电压","VDDA_ADC_3P3"]
[44,null,"GND","系统地"]
[45,"K14","UART1_TXD","串口1 TXD","UART1_TX_DATA","UART1_TX","ENET1_RDATA02","I2C3_SCL","CSI_DATA02","GPT1_COMPARE1","GPIO1_IO16",null,null,"SPDIF_OUT","UART5_TX(ULL)"]
[46,"K16","UART1_RXD","串口1 RXD","UART1_RX_DATA","UART1_RX","ENET1_RDATA03","I2C3_SDA","CSI_DATA03","GPT1_CLK","GPIO1_IO17",null,null,"SPDIF_IN","UART5_RX(ULL)"]
[47,"J17","UART2_TXD","串口2 TXD","UART2_TX_DATA","UART2_TX","ENET1_TDATA02","I2C4_SCL","CSI_DATA06","GPT1_CAPTURE1","GPIO1_IO20",null,null,"ECSPI3_SS0"]
[48,"J16","UART2_RXD","串口2 RXD","UART2_RX_DATA","UART2_RX","ENET1_TDATA03","I2C4_SDA","CSI_DATA07","GPT1_CAPTURE2","GPIO1_IO21",null,"SJC_DONE","ECSPI3_SCLK"]
[49,"H17","UART3_TXD","串口3 TXD","UART3_TX_DATA","UART3_TX","ENET2_RDATA02","SIM1_PORT0_PD(UL)","CSI_DATA01","UART2_CTS_B","GPIO1_IO24",null,"SJC_JTAG_ACT","ANATOP_OTG1_ID(ULL)"]
[50,"H16","UART3_RXD","串口3 RXD","UART3_RX_DATA","UART3_RX","ENET2_RDATA03",null,"CSI_DATA00","UART2_RTS_B","GPIO1_IO25",null,null,"EPIT1_OUT"]
[51,"G17","UART4_TXD","串口4 TXD","UART4_TX_DATA","UART4_TX","ENET2_TDATA02","I2C1_SCL","CSI_DATA12","CSU_CSU_ALARM_AUT02","GPIO1_IO28",null,null,"ECSPI2_SCLK"]
[52,"G16","UART4_RXD","串口4 RXD","UART4_RX_DATA","UART4_RX","ENET2_TDATA03","I2C1_SDA","CSI_DATA13","CSU_CSU_ALARM_AUT01","GPIO1_IO29",null,null,"ECSPI2_SS0","EPDC_PWRCTRL01(ULL)"]
[53,"F17","I2C2_SCL","I2C2时钟","UART5_TX_DATA","UART5_TX","ENET2_CRS","I2C2_SCL","CSI_DATA14","CSU_CSU_ALARM_AUT00","GPIO1_IO30",null,null,"ECSPI2_MOSI","EPDC_PWRCTRL02(ULL)"]
[54,"G13","I2C2_SDA","I2C2数据","UART5_RX_DATA","UART5_RX","ENET2_COL","I2C2_SDA","CSI_DATA15","CSU_CSU_INT_DEB","GPIO1_IO31",null,null,"ECSPI2_MISO","EPDC_PWRCTRL03(ULL)"]
[55,"L17","TS_XN","触摸屏XN","GPIO1_IO03","I2C1_SDA","GPT1_COMPARE3","USB_OTG2_OC","OSC32K_32K_OUT(UL)","USDHC1_CD_B","GPIO1_IO03","CCM_DI0_EXT_CLK","SRC_TESTER_ACK","UART1_RX"]
[56,"M16","TS_XP","触摸屏XP","GPIO1_IO04","ENET1_REF_CLK1","PWM3_OUT","USB_OTG1_PWR","ANATOP_24M_OUT(UL)","USDHC1_RESET_B","GPIO1_IO04","ENET2_1588_EVENT0_IN",null,"UART5_TX"]
[57,"L15","TS_YN","触摸屏YN","GPIO1_IO01","I2C2_SDA","GPT1_COMPARE1","USB_OTG1_OC","ENET2_REF_CLK2","MQS_LEFT","GPIO1_IO01","ENET1_1588_EVENT0_OUT","SRC_EARLY_RESET","WDOG1_WDOG_B"]
[58,"L14","TS_YP","触摸屏YP","GPIO1_IO02","I2C1_SCL","GPT1_COMPARE2","USB_OTG2_PWR","ENET1_REF_CLK_25M","USDHC1_WP","GPIO1_IO02","SDMA_EXT_EVENT00","SRC_ANY_PU_RESET","UART1_TX"]
[59,null,"GND","系统地"]
[60,null,"VDD_COIN_3V","备份电池电源输入","SNVS备份电池输入，正常可不接"]
[]
["注：红色标明的引脚针对I.MX6UL和I.MX6ULL处理器有差异"]