{"text_format":"3","workbook":"xlsx","n_sheets":4,"sheets":["RK-AIC技术规格","最小系统供电","接口资源分配","RK3568 IO资源分配"],"read":"whole","date_system":"1900"}

{"sheet":"RK-AIC技术规格","index":0,"n_rows":27,"n_cols":5,"rows_kept":27,"merged":[[0,1,0,3],[1,1,6,1],[7,1,9,1],[12,1,13,1],[14,1,15,1],[16,1,24,1]]}
[null,"RK-AIC 技术规格"]
[null,"最小系统","CPU","RK3568J工业级处理器，\n64Bit四核A55,主频2GHz","备注"]
[null,null,"GPU","Mali-G52-2EE, 800MHz"]
[null,null,"NPU","Up to 0.8TOPS"]
[null,null,"CPU RAM","DDR4, 4GB "]
[null,null,"Memory","eMMC5.1, 32GB "]
[null,null,"扩展算力卡","miniPCIe，默认PCIe 3.0 x 1line","可选PCIe2.1 RK1808算力卡，3.0 TOPS x 1"]
[null,"显示接口","LCD","默认10.1英寸TFT LCD，1280*800 Pixels"]
[null,null,"TP","10.1英寸电容多点触摸屏"]
[null,null,"HDMI OUT","HDMI 2.0,支持4K@60fps输出"]
[null,"Camera","Camera","MIPI-CSI 4lane * 1\n（或 MIPI-CSI 2lane * 2）"]
[null,"Audio","Audio","立体声音频输出，10W*2"]
[null,"通信","有线以太网","10/100/1000M Ethernet x 2"]
[null,null,"无线通信","4G/5G/WiFi-6，三选一"]
[null,"USB","USB3.0","USB3.0 OTG x 1"]
[null,null,"USB2.0","USB2.0 Device x 1\nUSB2.0 Host x 2"]
[null,"外设接口","CAN","CAN x 2"]
[null,null,"RS-232","RS-232 x 2"]
[null,null,"RS-485","RS-485 x 1"]
[null,null,"模拟量输入","4～20mA x 4\n0～5V x 4","默认 ARM Cortex-M3  控制"]
[null,null,"数字输入","Din x 4， NPN/PNP可配置","默认 ARM Cortex-M3  控制"]
[null,null,"数字输出","Dout x 4， NPN/PNP可配置","默认 ARM Cortex-M3  控制"]
[null,null,"继电器输出","SPST x 2"]
[null,null,"RGB三色灯","RGB三色灯 x 1"]
[null,null,"蜂鸣器","外置蜂鸣器 x 1"]
[null,"系统供电","系统供电","DC 12～24V"]
[null,"工作温度","工作温度","RK3568J：-40℃～85℃"]

{"sheet":"最小系统供电","index":1,"n_rows":40,"n_cols":7,"rows_kept":40}
[{"$nulls":3},"最小系统供电"]
[null,"页码","元件","受电网络","供电网络","电压","磁珠"]
[null,12,"RK3568-G","PMUIO1","VCC3V3_PMU",3.3,"FB1212"]
[{"$nulls":3},"PMUIO2","VCC3V3_PMU",3.3,"FB1236"]
[{"$nulls":3},"VDD_PMU_LOGIC_0V9","VDDA0V9_PMU",0.9,"FB1239"]
[{"$nulls":3},"PMUPLL_AVDD_0V9","VDDA0V9_PMU",0.9,"FB1214"]
[{"$nulls":3},"PMUPLL_AVDD_1V8","VDDA1V8_PMU",1.8,"FB1226"]
[{"$nulls":3},"SYSPLL_AVDD_0V9","VDDA_0V9",0.9,"FB1235"]
[{"$nulls":3},"SYSPLL_AVDD_1V8","VCCA_1V8",0.8,"FB1238"]
[null,13,"RK3568-I","VCCIO2","VCC_1V8",1.8,"FB1312"]
[null,null,"RK3568-J","VCCIO3","VCCIO_SD",3.3,"FB1315"]
[null,14,"RK3568-U","USB3_AVDD_0V9","VDDA_0V9",0.9,"FB1400"]
[{"$nulls":3},"USB3_AVDD_1V8","VCCA_1V8",1.8,"FB1402"]
[{"$nulls":3},"USB3_AVDD_3V3","VCC_3V3",3.3,"FB1404"]
[{"$nulls":3},"MULTI_PHY_AVDD_0V9","VDDA_0V9",0.9,"短接"]
[{"$nulls":3},"MULTI_PHY_AVDD_1V8","VCCA_1V8",1.8,"短接"]
[null,null,"RK3568-V","USB2_AVDD_0V9","VDDA_0V9",0.9,"FB1401"]
[{"$nulls":3},"USB2_AVDD_1V8","VCCA_1V8",1.8,"FB1403"]
[{"$nulls":3},"USB2_AVDD_3V3","VCC_3V3",3.3,"FB1405"]
[null,null,"RK3568-W","PCIE30_AVDD_0V9","VDDA_0V9",0.9,"短接"]
[{"$nulls":3},"PCIE30_AVDD_1V8","VCCA_1V8",1.8,"短接"]
[null,15,"RK3568-K","VCCIO4","VCC_1V8",1.8,"FB1518"]
[null,null,"RK3568-O","SARADC_AVDD_1V8","VCCA_1V8",1.8,"FB1514"]
[{"$nulls":3},"OTP_VCC18","VCC_1V8",1.8,"FB1517"]
[null,null,"RK3568-N","VCCIO7","VCC_3V3",3.3,"FB1576"]
[null,16,"RK3568-P","MIPI_AVDD_0V9","VDDA0V9_IMAGE",0.9,"FB1613"]
[{"$nulls":3},"MIPI_AVDD_1V8","VCCA1V8_IMAGE",1.8,"FB1618"]
[null,null,"RK3568-M","VCCIO6","VCC_1V8",1.8,"FB1670"]
[null,17,"RK3568-R","MIPI_DSI_TX0/LVDS_TX0_AVDD_0V9","VDDA0V9_IMAGE",0.9,"短接"]
[{"$nulls":3},"MIPI_DSI_TX0/LVDS_TX0_AVDD_1V8","VCCA1V8_IMAGE",1.8,"短接"]
[null,null,"RK3568-S","MIPI_DSI_TX1_AVDD_0V9","GND",0,"/"]
[{"$nulls":3},"MIPI_DSI_TX1_AVDD_1V8","GND",0,"/"]
[null,null,"RK3568-T","eDP_TX_AVDD_0V9","GND",0,"/"]
[{"$nulls":3},"eDP_TX_AVDD_1V8","GND",0,"/"]
[null,null,"RK3568-Q","HDMI_TX_AVDD_0V9","VDDA0V9_IMAGE",0.9,"短接"]
[{"$nulls":3},"HDMI_TX_AVDD_1V8","VCCA1V8_IMAGE",1.8,"短接"]
[null,18,"RK3568-L","VCCIO5","VCC_3V3","3.3V","短接"]
[null,19,"RK3568-H","VCCIO1","VCCIO_ACODEC","3.3V","短接"]
[null,23,"Flash Power Manage","VCCIO_FLASH","VCC_1V8",1.8,"FB2302"]
[{"$nulls":3},"VCC3V3_FLASH","VCC_3V3",3.3,"FB2305"]

{"sheet":"接口资源分配","index":2,"n_rows":26,"n_cols":6,"rows_kept":26}
[]
[{"$nulls":4},"USB资源分配"]
[null,null,"序号","MCU资源","连接器","用途"]
[null,null,"USB0","USB3.0 OTG","USB3.0 Type-A","用于固件升级，USB3.0 Device Type-A接口"]
[null,null,"USB1","USB3.0 HOST","板内","连接4G/5G模块，板内M.2接口"]
[null,null,"USB2","USB2.0 HOST","USB2.0 Type-A接口"]
[null,null,"USB3","USB2.0 HOST","USB2.0 Type-A接口"]
[]
[{"$nulls":4},"UART资源分配"]
[null,null,"序号","MCU资源","电平","用途"]
[null,null,"UART0"]
[null,null,"UART1"]
[null,null,"UART2","UART2_M0","3.3V","USB To UART for Debug"]
[null,null,"UART3","UART3_M1","3.3V","RS-232-0"]
[null,null,"UART4","UART4_M1","3.3V","RS-232-1"]
[null,null,"UART5","UART5_M0","3.3V","USE AS CAN0_M1"]
[null,null,"UART6","UART6_M1","3.3V","ARM Cortex-M3"]
[null,null,"UART7"]
[null,null,"UART8","UART8_M0","1.8V","Security MCU"]
[null,null,"UART9","UART9_M1","3.3V","RS-485"]
[]
[{"$nulls":4},"CAN资源分配"]
[null,null,"序号","MCU资源","电平","用途"]
[null,null,"CAN0","CAN0_M1","3.3V","CAN BUS 0"]
[null,null,"CAN1","CAN1_M1","3.3V","CAN BUS 1"]
[null,null,"CAN2","CAN2_M1","3.3V","Reserved"]

{"sheet":"RK3568 IO资源分配","index":3,"n_rows":132,"n_cols":19,"rows_kept":132,"merged":[[3,5,3,6],[3,7,3,8],[3,9,3,11]]}
[]
[{"$nulls":5},"RK3568 IO资源分配"]
[]
[{"$nulls":5},"RK_EVB1_RK3568",null,"RK智能控制器",null,"供电管脚"]
["页码","模块","CPU脚","功能模块","万象奥科","网络标号","应用","网络标号","应用","供电管脚","供电网络","电平(V)","功能","功能一","功能二","功能三","功能四","功能五","功能六"]
[11,"F",null,"DDR_PHY",null,null,"DDR4 PHY","DDR4 PHY","DDR4 PHY","VCC_DDR","VCC_DDR",1.21,"DDR4"]
[12,"G","AE26","PMUPLL",null,"RTCIC_INT_L_GPIO0_D3","RTC","TP1218","NC, 新RTC无中断引脚","PMUPLL_AVDD_1V8","VCCA1V8_PMU",1.8,"GPIO0_D3_d"]
[12,"G","AB23","PMUPLL",null,"PCIE_PWREN_H_GPIO0_D4",null,"PCIE_PWREN_H_GPIO0_D4","mini PCIe","PMUPLL_AVDD_1V8","VCCA1V8_PMU",1.8,"GPIO0_D4_d"]
[12,"G","AD25","PMUPLL",null,"VGA_PWREN_H_GPIO0_D5","VO-VGA Output","RK_DOUT_CTRL_GPIO0_D5","RK Dout *4 Channels","PMUPLL_AVDD_1V8","VCCA1V8_PMU",1.8,"GPIO0_D5_d"]
[12,"G","AC24","PMUPLL",null,"TP1215",null,"TP1215","NC, 备用Recovery Key","PMUPLL_AVDD_1V8","VCCA1V8_PMU",1.8,"GPIO0_D6_d"]
[12,"G","AG27","PMUIO1",null,"REFCLK_OUT_CAM",null,"REFCLK_OUT_CAM","Camera: MIPI-CSI","PMUIO1","VCC3V3_PMU",3.3,"GPIO0_A0_d"]
[12,"G","AG26","PMUIO1",null,"TSADC_SHUT_M0",null,"TSADC_SHUT_M0","RK3568_G: NPOR_u","PMUIO1","VCC3V3_PMU",3.3,"GPIO0_A1_d"]
[12,"G","AG28","PMUIO1",null,"PMIC_SLEEP_H",null,"PMIC_SLEEP_H","PMIC RK809 Managerment","PMUIO1","VCC3V3_PMU",3.3,"GPIO0_A2_d"]
[12,"G","AA22","PMUIO1",null,"PMIC_INT_L",null,"PMIC_INT_L","PMIC RK809 Managerment","PMUIO1","VCC3V3_PMU",3.3,"GPIO0_A3_d"]
[12,"G","Y22","PMUIO1",null,"SDMMC0_DET_L","MicroSD Card","RK_DOUT_0_GPIO0_A4","RK Dout *4 Channels","PMUIO1","VCC3V3_PMU",3.3,"GPIO0_A4_d"]
[12,"G","AF25","PMUIO1",null,"USB_OTG_PWREN_H_GPIO0_A5",null,"USB_OTG_PWREN_H_GPIO0_A5","USB 3.0 OTG","PMUIO1","VCC3V3_PMU",3.3,"GPIO0_A5_d"]
[12,"G","AE24","PMUIO1",null,"USB_HOST_PWREN_H_GPIO0_A6",null,"USB_HOST_PWREN_H_GPIO0_A6","USB 2.0 Host","PMUIO1","VCC3V3_PMU",3.3,"GPIO0_A6_d"]
[12,"G","AG25","PMUIO1",null,"FLASH_VOL_SEL",null,"FLASH_VOL_SEL","Flash Power Manage","PMUIO1","VCC3V3_PMU",3.3,"GPIO0_A7_d"]
[12,"G","AD23","PMUIO2",null,"CLK32K_OUT0_WIFI","WIFI/BT","RK_DOUT_1_GPIO0_B0","RK Dout *4 Channels","PMUIO2","VCC3V3_PMU",3.3,"GPIO0_B0_u"]
[12,"G","AF24","PMUIO2",null,"I2C0_SCL_PMIC",null,"I2C0_SCL_PMIC","PMIC RK809 Managerment","PMUIO2","VCC3V3_PMU",3.3,"GPIO0_B1_u"]
[12,"G","AB21","PMUIO2",null,"I2C0_SDA_PMIC",null,"I2C0_SDA_PMIC","PMIC RK809 Managerment","PMUIO2","VCC3V3_PMU",3.3,"GPIO0_B2_u"]
[12,"G","AG24","PMUIO2",null,"I2C1_SCL_TP",null,"I2C1_SCL_TP","Touch Panel","PMUIO2","VCC3V3_PMU",3.3,"GPIO0_B3_u"]
[12,"G","AB20","PMUIO2",null,"I2C1_SDA_TP",null,"I2C1_SDA_TP","Touch Panel","PMUIO2","VCC3V3_PMU",3.3,"GPIO0_B4_u"]
[12,"G","AC22","PMUIO2",null,"TP_INT_L_GPIO0_B5",null,"TP_INT_L_GPIO0_B5","Touch Panel","PMUIO2","VCC3V3_PMU",3.3,"GPIO0_B5_u"]
[12,"G","AA20","PMUIO2",null,"TP_RST_L_GPIO0_B6",null,"TP_RST_L_GPIO0_B6","Touch Panel","PMUIO2","VCC3V3_PMU",3.3,"GPIO0_B6_u"]
[12,"G","AH26","PMUIO2",null,"CPU_AVS/CPU_DVS_PWM0_M0","VDD_CPU_EXT","TP1219","NC, 无VDD_CPU_EXT","PMUIO2","VCC3V3_PMU",3.3,"GPIO0_B7_u"]
[12,"G","AD22","PMUIO2",null,"WORKING_LEDEN_H_GPIO0_C0",null,"WORKING_LEDEN_H_GPIO0_C0","Working LED","PMUIO2","VCC3V3_PMU",3.3,"GPIO0_C0_d"]
[12,"G","AF23","PMUIO2",null,"DVP_PWREN0_H_GPIO0_C1",null,"DVP_PWREN0_H_GPIO0_C1","Camera: MIPI-CSI","PMUIO2","VCC3V3_PMU",3.3,"GPIO0_C1_d"]
[12,"G","AG23","PMUIO2",null,"EDP_HPDIN_M1","VO-VGA Output","LED_OUT1_PWM3_IR","Dout for LED*3","PMUIO2","VCC3V3_PMU",3.3,"GPIO0_C2_d","PWM3_IR"]
[12,"G","AE23","PMUIO2",null,"LCD0_BL_PWM4",null,"LCD0_BL_PWM4","MIPI_DSI_TX0/LVDS_TX0","PMUIO2","VCC3V3_PMU",3.3,"GPIO0_C3_d","PWM4"]
[12,"G","AD21","PMUIO2",null,"LCD1_BL_PWM5","VO-LCM_MIPI-DSI_TX1","LED_OUT2_PWM5","Dout for LED*3","PMUIO2","VCC3V3_PMU",3.3,"GPIO0_C4_d","PWM5"]
[12,"G","AC21","PMUIO2",null,"LCD1_PWREN_H_GPIO0_C5","VO-LCM_MIPI-DSI_TX1","LCD0_RST_L_GPIO0_C5","MIPI_DSI_TX0/LVDS_TX0","PMUIO2","VCC3V3_PMU",3.3,"GPIO0_C5_d"]
[12,"G","AD20","PMUIO2",null,"PWM7_IR","IR Receiver","LED_OUT3_PWM7_IR","Dout for LED*3","PMUIO2","VCC3V3_PMU",3.3,"GPIO0_C6_d","PWM7_IR"]
[12,"G","AH25","PMUIO2",null,"LCD0_PWREN_H_GPIO0_C7",null,"LCD0_PWREN_H_GPIO0_C7","MIPI_DSI_TX0/LVDS_TX0","PMUIO2","VCC3V3_PMU",3.3,"GPIO0_C7_d"]
[12,"G","AC20","PMUIO2",null,"UART2_RX_M0_DEBUG",null,"UART2_RX_M0_DEBUG","UART2_M0 For Debug","PMUIO2","VCC3V3_PMU",3.3,"GPIO0_D0_u","UART2_RX_M0"]
[12,"G","AH24","PMUIO2",null,"UART2_TX_M0_DEBUG",null,"UART2_TX_M0_DEBUG","UART2_M0 For Debug","PMUIO2","VCC3V3_PMU",3.3,"GPIO0_D1_u","UART2_TX_M0"]
[13,"I",null,"eMMC Flash Controller",null,null,"eMMC Flash Controller",null,"eMMC Flash Controller","VCCIO2","VCCIO_FLASH",1.8]
[13,"J","J25","SD Controlle",null,"SDMMC0_D0/UART2_TX_M1/UART6_TX_M1/PWM8_M1","MicroSD Card/UART6","UART6_TX_M1","ARM Cortex-M3","VCCIO3","VCCIO_SD",3.3,"GPIO1_D5_u","UART6_TX_M1","SDMMC0_D0","PWM8_M1"]
[13,"J","J24","SD Controlle",null,"SDMMC0_D1/UART2_RX_M1/UART6_RX_M1/PWM9_M1","MicroSD Card/UART6","UART6_RX_M1","ARM Cortex-M3","VCCIO3","VCCIO_SD",3.3,"GPIO1_D6_u","UART6_RX_M1","SDMMC0_D1","PWM9_M1"]
[13,"J","H26","SD Controlle",null,"SDMMC0_D2/ARMJTAG_TCK","MicroSD Card/ARMJTAG","ARMJTAG_TCK","ARMJTAG","VCCIO3","VCCIO_SD",3.3,"GPIO1_D7_u","ARMJTAG_TCK","SDMMC0_D2"]
[13,"J","J23","SD Controlle",null,"SDMMC0_D3/ARMJTAG_TMS","MicroSD Card/ARMJTAG","ARMJTAG_TMS","ARMJTAG","VCCIO3","VCCIO_SD",3.3,"GPIO2_A0_u","ARMJTAG_TMS","SDMMC0_D3"]
[13,"J","H27","SD Controlle",null,"SDMMC0_CMD/PWM10_M1/UART5_RX_M0/CAN0_TX_M1","MicroSD Card/UART5/CAN0","CAN0_TX_M1","CAN0","VCCIO3","VCCIO_SD",3.3,"GPIO2_A1_u","CAN0_TX_M1","SDMMC0_CMD","UART5_RX_M0"]
[13,"J","H28","SD Controlle",null,"SDMMC0_CLK/TEST_CLKOUT/UART5_TX_M0/CAN0_RX_M1","MicroSD Card/UART5/CAN0","CAN0_RX_M1","CAN0","VCCIO3","VCCIO_SD",3.3,"GPIO2_A2_d","CAN0_RX_M1","SDMMC0_CLK","UART5_TX_M0"]
[14,"U",null,"USB 3.0 OTG0",null,null,"USB 3.0 OTG0 -> USB Download",null,"USB 3.0 OTG0 -> USB Download"]
[14,"U",null,"USB 3.0 Host1",null,null,"USB 3.0 Host1",null,"USB 3.0 Host1 -> M.2 4G and 5G Module"]
[14,"U",null,"PCIe2.0 and SATA2",null,null,"SATA3.0 Port2",null,"PCIe2.0 -> mini PCIe"]
[14,"U",null,"MULTI_PHY REFCLK",null,null,"PCIe3.0 x 2Lanes",null,"NC"]
[14,"V",null,"USB2.0 HOST",null,null,"USB2.0 HOST",null,"USB2.0 HOST"]
[14,"W",null,"PCIe3.0 x2",null,null,"PCIe3.0 x2",null,"PCIe3.0 x1 -> mini PCIe"]
[15,"K",null," GMAC0",null,null," GMAC0",null," GMAC0","VCCIO4","VCC_1V8",1.8]
[15,"K","D26","UART / CAN",null,"UART8_RTSn_M0","WIFI/BT","CAN2_RX_M1","CAN2_M1, 预留","VCCIO4","VCC_1V8",1.8,"GPIO2_B1_d","CAN2_RX_M1","UART8_RTSn_M0"]
[15,"K","E25","UART / CAN",null,"UART8_CTSn_M0","WIFI/BT","CAN2_TX_M1","CAN2_M1, 预留","VCCIO4","VCC_1V8",1.8,"GPIO2_B2_u","CAN2_TX_M1","UART8_CTSn_M0"]
[15,"K","F26","UART / CAN",null,"UART8_TX_M0","WIFI/BT","UART8_TX_M0","Security MCU UART","VCCIO4","VCC_1V8",1.8,"GPIO2_C5_d","UART8_TX_M0"]
[15,"K","E26","UART / CAN",null,"UART8_RX_M0","WIFI/BT","UART8_RX_M0","Security MCU UART","VCCIO4","VCC_1V8",1.8,"GPIO2_C6_d","UART8_RX_M0"]
[15,"N","AF8","CAN",null,"CAN1_RX_M1",null,"CAN1_RX_M1","CAN1","VCCIO7","VCC_3V3",3.3,"GPIO4_C2_d","CAN1_RX_M1"]
[15,"N","AA11","CAN",null,"CAN1_TX_M1",null,"CAN1_TX_M1","CAN1","VCCIO7","VCC_3V3",3.3,"GPIO4_C3_d","CAN1_TX_M1"]
[15,"N","AH7","GPIO",null,"SATA2_ACT_LED","SATA3.0 Port2","RK_DOUT_2_GPIO4_C4","RK Dout *4 Channels","VCCIO7","VCC_3V3",3.3,"GPIO4_C4_d","SATA2_ACT_LED"]
[15,"N","AD8","UART",null,"UART9_TX_M1","UART/CAN Port","UART9_TX_M1","RS-485","VCCIO7","VCC_3V3",3.3,"GPIO4_C5_d","UART9_TX_M1"]
[15,"N","AE8","UART",null,"UART9_RX_M1","UART/CAN Port","UART9_RX_M1","RS-485","VCCIO7","VCC_3V3",3.3,"GPIO4_C6_d","UART9_RX_M1"]
[15,"N","AG8","HDMI2.0 TX",null,"HDMITX_SCL",null,"HDMITX_SCL","HDMI2.0 TX","VCCIO7","VCC_3V3",3.3,"GPIO4_C7_u","HDMITX_SCL"]
[15,"N","AG7","HDMI2.0 TX",null,"HDMITX_SDA",null,"HDMITX_SDA","HDMI2.0 TX","VCCIO7","VCC_3V3",3.3,"GPIO4_D0_u","HDMITX_SDA"]
[15,"N","AH6","HDMI2.0 TX",null,"HDMITX_CEC_M0",null,"HDMITX_CEC_M0","HDMI2.0 TX","VCCIO7","VCC_3V3",3.3,"GPIO4_D1_u","HDMITX_CEC_M0"]
[15,"N","AB9","GPIO",null,"CON_INT_L_GPIO4_D2","CIF,EBC,RGMII,BT656","RS485_TX_EN_L_GPIO4_D2","RS-485","VCCIO7","VCC_3V3",3.3,"GPIO4_D2_u"]
[15,"O","B27","SARADC/OTP",null,"SARADC_VIN0_KEY/RECOVERY","KEY Array","SARADC_VIN0","Recovery Key or Ain Optional","SARADC_AVDD_1V8","VCCA_1V8",1.8,"SARADC_VIN0"]
[15,"O","C26","SARADC/OTP",null,"SARADC_VIN1_EVB_HW_ID","EVB_HW_ID","SARADC_VIN1","EVB_HW_ID or Ain Optional","SARADC_AVDD_1V8","VCCA_1V8",1.8,"SARADC_VIN1"]
[15,"O","D24","SARADC/OTP",null,"SARADC_VIN2_LCD_ID","LCD_ID","SARADC_VIN2","LCD_ID or Ain Optional","SARADC_AVDD_1V8","VCCA_1V8",1.8,"SARADC_VIN2"]
[15,"O","E23","SARADC/OTP",null,"SARADC_VIN3","Connector：J9200","SARADC_VIN3","24V ADC or Ain Optional","SARADC_AVDD_1V8","VCCA_1V8",1.8,"SARADC_VIN3"]
[15,"O","G21","SARADC/OTP",null,"SARADC_VIN4","Connector：J9200","SARADC_VIN4","Ain: 4～20mA, Optional","SARADC_AVDD_1V8","VCCA_1V8",1.8,"SARADC_VIN4"]
[15,"O","F22","SARADC/OTP",null,"SARADC_VIN5","Connector：J9200","SARADC_VIN5","Ain: 4～20mA, Optional","SARADC_AVDD_1V8","VCCA_1V8",1.8,"SARADC_VIN5"]
[15,"O","G20","SARADC/OTP",null,"SARADC_VIN6","Connector：J9200","SARADC_VIN6","Ain: 0～5V, Optional","SARADC_AVDD_1V8","VCCA_1V8",1.8,"SARADC_VIN6"]
[15,"O","F21","SARADC/OTP",null,"SARADC_VIN7","Connector：J9200","SARADC_VIN7","Ain: 0～5V, Optional","SARADC_AVDD_1V8","VCCA_1V8",1.8,"SARADC_VIN7"]
[16,"P",null,"MIPI_CSI_RX",null,null,"MIPI_CSI_RX",null,"MIPI_CSI_RX","MIPI_CSI_RX_AVDD_0V9/MIPI_CSI_RX_AVDD_1V8","VDDA0V9_IMAGE/VDDA1V8_IMAGE","0.9/1.8"]
[16,"M","AC5","GPIO3",null,"SDMMC2_D0_M0","WIFI/BT","N32_RESET_L_GPIO3_C6","Security MCU Reset","VCCIO6","VCC_1V8",1.8,"GPIO3_C6_d"]
[16,"M","AA6","GPIO3",null,"SDMMC2_D1_M0","WIFI/BT","ARM_M3_RESET_L_GPIO3_C7","ARM Cortex-M3 Reset","VCCIO6","VCC_1V8",1.8,"GPIO3_C7_d"]
[16,"M","AB5","GPIO3",null,"SDMMC2_D2_M0","WIFI/BT","4G_CFG0_GPIO3_D0","M.2 4G/5G Module CFG","VCCIO6","VCC_1V8",1.8,"GPIO3_D0_d"]
[16,"M","AB1","GPIO3",null,"SDMMC2_D3_M0","WIFI/BT","4G_CFG1_GPIO3_D1","M.2 4G/5G Module CFG","VCCIO6","VCC_1V8",1.8,"GPIO3_D1_d"]
[16,"M","Y7","GPIO3",null,"SDMMC2_CMD_M0","WIFI/BT","4G_CFG2_GPIO3_D2","M.2 4G/5G Module CFG","VCCIO6","VCC_1V8",1.8,"GPIO3_D2_d"]
[16,"M","AC1","GPIO3",null,"SDMMC2_CLK_M0","WIFI/BT","4G_CFG3_GPIO3_D3","M.2 4G/5G Module CFG","VCCIO6","VCC_1V8",1.8,"GPIO3_D3_d"]
[16,"M","AA1","GPIO3",null,"WIFI_WAKE_HOST_H_GPIO3_D4","WIFI/BT","RELAY1_L_GPIO3_D4","Relay*2","VCCIO6","VCC_1V8",1.8,"GPIO3_D4_d"]
[16,"M","AA5","GPIO3",null,"WIFI_REG_ON_H_GPIO3_D5","WIFI/BT","RELAY2_L_GPIO3_D5","Relay*2","VCCIO6","VCC_1V8",1.8,"GPIO3_D5_d"]
[16,"M",null,"GMAC1",null,null,"GMAC1",null,"GMAC1","VCCIO6","VCC_1V8",1.8]
[16,"M","V1","GPIO4",null,"I2C4_SDA_M0",null,"I2C4_SDA_M0","Camera: MIPI-CSI","VCCIO6","VCC_1V8",1.8,"GPIO4_B2_d","I2C4_SDA_M0"]
[16,"M","V4","GPIO4",null,"I2C4_SCL_M0",null,"I2C4_SCL_M0","Camera: MIPI-CSI","VCCIO6","VCC_1V8",1.8,"GPIO4_B3_d","I2C4_SCL_M0"]
[16,"M","V6","GPIO4",null,"CAMERA0_PDN_L_GPIO4_B4",null,"CAMERA0_PDN_L_GPIO4_B4","Camera: MIPI-CSI","VCCIO6","VCC_1V8",1.8,"GPIO4_B4_d","I2C2_SDA_M1"]
[16,"M","V5","GPIO4",null,"CAMERA1_PDN_L_GPIO4_B5",null,"CAMERA1_PDN_L_GPIO4_B5","Camera: MIPI-CSI","VCCIO6","VCC_1V8",1.8,"GPIO4_B5_d","I2C2_SCL_M1"]
[16,"M","U3","GPIO4",null,"CIF_CLKOUT",null,"CIF_CLKOUT","Camera: MIPI-CSI","VCCIO6","VCC_1V8",1.8,"GPIO4_C0_d"]
[17,"R",null,"MIPI_DSI_TX0/LVDS_TX0",null,null,"MIPI_DSI_TX0/LVDS_TX0",null,"MIPI_DSI_TX0/LVDS_TX0","LVDS_TX0_AVDD_0V9/LVDS_TX0_AVDD_1V8","VDDA0V9_IMAGE/VCCA1V8_IMAGE","0.9/1.8"]
[17,"S",null,"MIPI_DSI_TX1",null,null,"MIPI_DSI_TX1",null,"NC","MIPI_DSI_TX1_AVDD_0V9/MIPI_DSI_TX1_AVDD_1V8","GND/GND",0]
[17,"T",null,"eDP TX",null,null,"eDP TX",null,"NC","eDP_TX_AVDD_0V9/eDP_TX_AVDD_1V8","GND/GND",0]
[17,"Q",null,"HDMI2.0 TX",null,null,"HDMI2.0 TX",null,"HDMI2.0 TX","HDMI_TX_AVDD_0V9/HDMI_TX_AVDD_1V8","VDDA0V9_IMAGE/VCCA1V8_IMAGE","0.9/1.8"]
[18,"L","AG6","GPIO2_D0_d",null,"GMAC1_INT/PMEB_GPIO2_D0",null,"GMAC1_INT/PMEB_GPIO2_D0","Ethernet 1","VCCIO5","VCC_3V3",3.3,"GPIO2_D0_d"]
[18,"L","AD7","GPIO2_D1_d",null,"GMAC1_RSTn_GPIO2_D1",null,"GMAC1_RSTN_GPIO2_D1","Ethernet 1","VCCIO5","VCC_3V3",3.3,"GPIO2_D1_d"]
[18,"L","AC8","GPIO2_D2_d",null,"GMAC0_INT/PMEB_GPIO2_D2",null,"GMAC0_INT/PMEB_GPIO2_D2","Ethernet 0","VCCIO5","VCC_3V3",3.3,"GPIO2_D2_d"]
[18,"L","AC7","GPIO2_D3_d",null,"GMAC0_RSTn_GPIO2_D3",null,"GMAC0_RSTN_GPIO2_D3","Ethernet 0","VCCIO5","VCC_3V3",3.3,"GPIO2_D3_d"]
[18,"L","AF5","GPIO2_D4_d",null,"PCIE30X2_CLKREQn_M1",null,"PCIE30X2_CLKREQN_M1","mini PCIe ( PCIe3.0 x 1Lanes )","VCCIO5","VCC_3V3",3.3,"GPIO2_D4_d"]
[18,"L","AF6","GPIO2_D5_d",null,"PCIE30X2_WAKEn_M1",null,"PCIE30X2_WAKEN_M1","mini PCIe ( PCIe3.0 x 1Lanes )","VCCIO5","VCC_3V3",3.3,"GPIO2_D5_d"]
[18,"L","AD6","GPIO2_D6_d",null,"PCIE30X2_PERSTn_M1",null,"PCIE30X2_PERSTN_M1","mini PCIe ( PCIe3.0 x 1Lanes )","VCCIO5","VCC_3V3",3.3,"GPIO2_D6_d"]
[18,"L","AH5","GPIO2_D7_d",null,"PCIE30X2_PRSNT_L_GPIO2_D7",null,"PCIE30X2_PRSNT_L_GPIO2_D7","mini PCIe ( PCIe3.0 x 1Lanes )","VCCIO5","VCC_3V3",3.3,"GPIO2_D7_d"]
[18,"L","AH4","GPIO3_A0_d",null,"BT_REG_ON_H_GPIO3_A0","WIFI/BT","4G_POWER_EN_L_GPIO3_A0","M.2 4G/5G Module Control","VCCIO5","VCC_3V3",3.3,"GPIO3_A0_d"]
[18,"L","AB8","GPIO3_A1_d",null,"BT_WAKE_HOST_H_GPIO3_A1","WIFI/BT","4G_POWER_KEY_L_GPIO3_A1","M.2 4G/5G Module Control","VCCIO5","VCC_3V3",3.3,"GPIO3_A1_d"]
[18,"L","AE5","GPIO3_A2_d",null,"HOST_WAKE_BT_H_GPIO3_A2","WIFI/BT","4G_RESET_L_GPIO3_A2","M.2 4G/5G Module Control","VCCIO5","VCC_3V3",3.3,"GPIO3_A2_d"]
[18,"L","AG4","GPIO3_A3_d",null,"I2S3_SCLK_M0","WIFI/BT","RK_DIN_0_GPIO3_A3","RK Din *4 Channels","VCCIO5","VCC_3V3",3.3,"GPIO3_A3_d"]
[18,"L","AF4","GPIO3_A4_d",null,"I2S3_LRCK_M0","WIFI/BT","RK_DIN_1_GPIO3_A4","RK Din *4 Channels","VCCIO5","VCC_3V3",3.3,"GPIO3_A4_d"]
[18,"L","AH3","GPIO3_A5_d",null,"I2S3_SDO_M0","WIFI/BT","RK_DIN_2_GPIO3_A5","RK Din *4 Channels","VCCIO5","VCC_3V3",3.3,"GPIO3_A5_d"]
[18,"L","AG3","GPIO3_A6_d",null,"I2S3_SDI_M0","WIFI/BT","RK_DIN_3_GPIO3_A6","RK Din *4 Channels","VCCIO5","VCC_3V3",3.3,"GPIO3_A6_d"]
[18,"L","AH2","GPIO3_A7_d",null,"PCIECLKIC_OE_H_GPIO3_A7",null,"PCIECLKIC_OE_H_GPIO3_A7","mini PCIe ( PCIe3.0 x 1Lanes )","VCCIO5","VCC_3V3",3.3,"GPIO3_A7_d"]
[18,"L","AG2","GPIO3_B0_d",null,"ETH1_REFCLKO_25M_M0",null,"ETH1_REFCLKO_25M_M0","Ethernet 0","VCCIO5","VCC_3V3",3.3,"GPIO3_B0_d"]
[18,"L","AG1","GPIO3_B1_d",null,"UART4_RX_M1","UART/CAN Port","UART4_RX_M1","RS-232-1","VCCIO5","VCC_3V3",3.3,"GPIO3_B1_d","UART4_RX_M1"]
[18,"L","AF2","GPIO3_B2_d",null,"UART4_TX_M1","UART/CAN Port","UART4_TX_M1","RS-232-1","VCCIO5","VCC_3V3",3.3,"GPIO3_B2_d","UART4_TX_M1"]
[18,"L","AF1","GPIO3_B3_d",null,"I2C5_SCL_M0","RTC, HYM8563TS","I2C5_SCL_M0","RTC，ISL1208","VCCIO5","VCC_3V3",3.3,"GPIO3_B3_d","I2C5_SCL_M0"]
[18,"L","AE1","GPIO3_B4_d",null,"I2C5_SDA_M0","RTC, HYM8563TS","I2C5_SDA_M0","RTC，ISL1208","VCCIO5","VCC_3V3",3.3,"GPIO3_B4_d","I2C5_SDA_M0"]
[18,"L","AE2","GPIO3_B5_d",null,"MIPICAM1_RST_L_GPIO3_B5",null,"MIPICAM1_RST_L_GPIO3_B5","Camera: MIPI-CSI","VCCIO5","VCC_3V3",3.3,"GPIO3_B5_d"]
[18,"L","AE3","GPIO3_B6_d",null,"MIPICAM0_RST_L_GPIO3_B6",null,"MIPICAM0_RST_L_GPIO3_B6","Camera: MIPI-CSI","VCCIO5","VCC_3V3",3.3,"GPIO3_B6_d"]
[18,"L","AD4","GPIO3_B7_d",null,"UART3_TX_M1","UART/CAN Port","UART3_TX_M1","RS-232-0","VCCIO5","VCC_3V3",3.3,"GPIO3_B7_d","UART3_TX_M1"]
[18,"L","AD2","GPIO3_C0_d",null,"UART3_RX_M1","UART/CAN Port","UART3_RX_M1","RS-232-0","VCCIO5","VCC_3V3",3.3,"GPIO3_C0_d","UART3_RX_M1"]
[18,"L","AD1","GPIO3_C1_d",null,"GSENSOR_INT_L_GPIO3_C1","Gyroscope+G-sensor","RK_DIN_CTRL_GPIO3_C1","RK Din *4 Channels","VCCIO5","VCC_3V3",3.3,"GPIO3_C1_d"]
[18,"L","AA7","GPIO3_C2_d",null,"HP_DET_L_GPIO3_C2","Headphone","AUDIO_PA_FAULT_L_GPIO3_C2","Audio Power Amplifier","VCCIO5","VCC_3V3",3.3,"GPIO3_C2_d"]
[18,"L","AC4","GPIO3_C3_d",null,"PA_EN_H_GPIO3_C3","Audio-MIC Array Interface","AUDIO_PA_SD_H_GPIO3_C3","Audio Power Amplifier","VCCIO5","VCC_3V3",3.3,"GPIO3_C3_d"]
[18,"L","AC3","GPIO3_C4_d",null,"PWM14_M0",null,"PWM14_M0","Camera: MIPI-CSI","VCCIO5","VCC_3V3",3.3,"GPIO3_C4_d","PWM14_M0"]
[18,"L","AC2","GPIO3_C5_d",null,"SPDIF_TX_M1","Audio-S/PDIF TX Port","BUZZER_PWM15_IR_M0","Buzzer","VCCIO5","VCC_3V3",3.3,"GPIO3_C5_d","PWM15_IR_M0"]
[19,"H","D18","GPIO1",null,"I2C3_SDA_M0","Audio-MIC Array Interface/CIF,EBC,RGMII,BT656","I2C3_SDA_M0","Camera: MIPI-CSI","VCCIO1","VCCIO_ACODEC",3.3,"GPIO1_A0_u","I2C3_SDA_M0"]
[19,"H","E18","GPIO1",null,"I2C3_SCL_M0","Audio-MIC Array Interface/CIF,EBC,RGMII,BT656","I2C3_SCL_M0","Camera: MIPI-CSI","VCCIO1","VCCIO_ACODEC",3.3,"GPIO1_A1_u","I2C3_SCL_M0"]
[19,"H","A19","GPIO1",null,"I2S1_MCLK_M0_RK809",null,"I2S1_MCLK_M0_RK809","PMIC RK809 CODEC","VCCIO1","VCCIO_ACODEC",3.3,"GPIO1_A2_d"]
[19,"H","B19","GPIO1",null,"I2S1_SCLK_TX_M0_RK809",null,"I2S1_SCLK_TX_M0_RK809","PMIC RK809 CODEC","VCCIO1","VCCIO_ACODEC",3.3,"GPIO1_A3_d"]
[19,"H","F18","GPIO1",null,"I2S1_SCLK_RX_M0/PDM_CLK1_M0","Audio-MIC Array Interface","RK_DOUT_3_GPIO1_A4","RK Dout *4 Channels","VCCIO1","VCCIO_ACODEC",3.3,"GPIO1_A4_d"]
[19,"H","A20","GPIO1",null,"I2S1_LRCK_TX_M0_RK809",null,"I2S1_LRCK_TX_M0_RK809","PMIC RK809 CODEC","VCCIO1","VCCIO_ACODEC",3.3,"GPIO1_A5_d"]
[19,"H","C20","GPIO1",null,"PDM_CLK0_M0_RK809",null,"PDM_CLK0_M0_RK809","PMIC RK809 CODEC","VCCIO1","VCCIO_ACODEC",3.3,"GPIO1_A6_d"]
[19,"H","B20","GPIO1",null,"I2S1_SDO0_M0_RK809",null,"I2S1_SDO0_M0_RK809","PMIC RK809 CODEC","VCCIO1","VCCIO_ACODEC",3.3,"GPIO1_A7_d"]
[19,"H","D20","GPIO1",null,"I2S1_SDO1_M0/I2S1_SDI3_M0/PDM_SDI3_M0","Audio-MIC Array Interface","PCIE20_CLKREQN_M2","mini PCIe ( PCIe2.0 x 1Lanes )","VCCIO1","VCCIO_ACODEC",3.3,"GPIO1_B0_d"]
[19,"H","E20","GPIO1",null,"I2S1_SDO2_M0/I2S1_SDI2_M0/PDM_SDI2_M0","Audio-MIC Array Interface","PCIE20_WAKEN_M2","mini PCIe ( PCIe2.0 x 1Lanes )","VCCIO1","VCCIO_ACODEC",3.3,"GPIO1_B1_d"]
[19,"H","A21","GPIO1",null,"I2S1_SDO3_M0/I2S1_SDI1_M0/PDM_SDI1_M0","Audio-MIC Array Interface","PCIE20_PERSTN_M2","mini PCIe ( PCIe2.0 x 1Lanes )","VCCIO1","VCCIO_ACODEC",3.3,"GPIO1_B2_d"]
[19,"H","B21","GPIO1",null,"I2S1_SDI0_M0/PDM_SDI0_M0_RK809",null,"I2S1_SDI0_M0/PDM_SDI0_M0_RK809","PMIC RK809 CODEC","VCCIO1","VCCIO_ACODEC",3.3,"GPIO1_B3_d"]